20190927 – Day 13

* Using the blue tubing and the drippers I made the new low flow system
  + Put tubing over the black end and put it onto the inflow nozzle. Works great and can remove if need be to flush lines!
  + The red/orange tip of the drippers faced out produced ½ Gallon per hr drip rate
* Started by emptying the reservoir and flushing 5 Gallons from the line
* Then cut pieces of tubing around the drippers so could get system up and running
* In the meantime, took measurements
  + Tanks all look cloudy and I am not sure why (TURNS out it is water stagnation).
* All light measurements low because sunset setting begun when started taking measurements
* Drippers left on over the weekend

Measurements seen on google/excel sheet